|  |  |  |
| --- | --- | --- |
| connellylogo | **Job Safety Analysis Worksheet** |  |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Contractor:** | Connelly & Associates, INC. |  | **Date:** | | | | | | **9/26/2013** | | |
|  |  |  | **Job Number** | | | | | |  | | |
|  |  |  | **Job Name** | | | | | |  | | |
| **Team Name:** |  |  |  | |  | | |
|  |  |  |  | | |  |  | | |  | |
| **Team Leader:** |  |  | **JSA team members:** | **Name** | | | **Initials** | | **Name** | | **Initials** |
|  |  |  |
| Description of work: | Operating Skid Steer |  | |  | | |  | |  | |  |
|  |  |  | |  | | |  | |  | |  |
|  |  |  | |  | | |  | |  | |  |
|  |  |  | |  | | |  | |  | |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Activity List the tasks required to perform the activity in the sequence they are carried out. | Hazards Against each task list the hazards that could cause injury when the task is performed. | Risk control measures List the control measures required to eliminate or minimize the risk of injury arising from the identified hazard. | Severity Ranking |
| 1. Safety check of unit. | Injury due to equipment failure. | Do not operate unit that has faulty parts or equipment. If a problem is found, contact supervisor to initiate repairs of any damage. Do not modify or bypass any safety devices. | 4 |
| 1. Mounting/dismounting equipment | Slips, trips and falls | Always establish 3 points of contact method when mounting or dismounting equipment. Only use verified factory installed steps and handles. Clear debris or dirt from steps if necessary | 4 |
| 1. Operating/moving equipment | Injury to pedestrians/workers or damage to equipment and injury from tip over. Crushing injury. | Keep arms, legs and head inside while skid steer while operating. Only trained and authorized employees may operate this equipment. Sound horn when entering buildings, approaching pedestrians or going around blind corners. Drive slowly and carefully with bucket or attachments low as possible. ALWAYS give right of way to the pedestrian or any piece of equipment or vehicle in your travel path. | 8 |
| 1. Loading, unloading and moving of materials | Load not positioned properly on bobcat and falls causing crushing injury | Never lift a load greater than unit capacity. When lifting load ensure load is securely positioned on to bobcat. | 4 |
| 1. Backing equipment | Struck by and/or crushing injury | Use extreme caution when backing. Blind spot exists on equipment therefore back up alarm must be in use.  Review “No Zone” exclusion areas with site workers. Distances of operator’s view will vary depending upon type of equipment being used. | 4 |
| 1. Manually moving or lifting unit attachments. | Back strain, pulled muscles | Use proper lifting methods and get assistance when needed. | 4 |